INSTRUCTIONS FOR FORM USE; ALTIMETER CALIBRATION AND TEST

1. Enter the Work Order number on which the work is being performed
2. Place an X in the box next to the position of the Altimeter
3. Enter the name of the Manufacturer of the Altimeter
4. Enter the Part number of the Altimeter
5. Enter the Model number of the Altimeter
6. Enter the Serial Number of the Altimeter
7. Enter the name of the Manufacturer of the Encoder or Air Data Computer
8. Enter the Encoder or Air Data Computer Part Number
9. Enter the Model of the Encoder or Air Data Computer
10. Enter the Serial Number of the Encoder or Air Data Computer
11. Enter the Scale Error next to each parameter
12. Enter the Barometric Scale Error next to each parameter
13. Enter the value of Hysteresis for each parameter
14. Enter the value of the Case Leak as tested
15. Enter the values for the three (3) parameters of the After Effect following the test
16. Enter the aircraft registration number
17. Enter the date on which the Altimeter Test was completed
18. Enter the Identification number of the test equipment used
19. Enter the name of the person who performed the Altimeter Test
20. Place employee initials in the boxes for each Inspection provess

NOTE: Not all fields always require text entry. Contact your supervisor if there are questions. In cases where data is not required, DO NOT leave blank; enter N/A.